<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.26" y2="0" width="0" layer="20"/>
<wire x1="21.26" y1="0" x2="21.26" y2="15.23" width="0" layer="20"/>
<wire x1="21.26" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="CC0402JRX7R7BB104">
<packages>
<package name="CAPC1005X55N">
</package>
</packages>
</library>
<library name="CC0603KRX7R7BB152">
<packages>
<package name="CAPC1608X90">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1_05X2MM">
<description>CON-M-1X5-200</description>
</package>
</packages>
</library>
<library name="RC0603JR-0710KL">
<packages>
<package name="RESC1607X60N">
</package>
</packages>
</library>
<library name="DRV5053PAQDBZR">
<packages>
<package name="SOT95P237X112-3N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="CC0402JRX7R7BB104" package="CAPC1005X55N" value="CC0402JRX7R7BB104">
<attribute name="DESCRIPTION" value=" Cap Ceramic 0.1uF 16V X7R 5% SMD 0402 125°C Paper T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-1676-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/CC0402JRX7R7BB104/311-1676-1-ND/5195578?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="CC0402JRX7R7BB104"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0402 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="CC0402JRX7R7BB104" package="CAPC1005X55N" value="CC0402JRX7R7BB104">
<attribute name="DESCRIPTION" value=" Cap Ceramic 0.1uF 16V X7R 5% SMD 0402 125°C Paper T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-1676-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/CC0402JRX7R7BB104/311-1676-1-ND/5195578?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="CC0402JRX7R7BB104"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0402 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="CC0402JRX7R7BB104" package="CAPC1005X55N" value="CC0402JRX7R7BB104">
<attribute name="DESCRIPTION" value=" Cap Ceramic 0.1uF 16V X7R 5% SMD 0402 125°C Paper T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-1676-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/CC0402JRX7R7BB104/311-1676-1-ND/5195578?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="CC0402JRX7R7BB104"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0402 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="CC0603KRX7R7BB152" package="CAPC1608X90" value="CC0603KRX7R7BB152">
<attribute name="DESCRIPTION" value=" 0603 1.5 nF 16 V ±10 % Tolerance X7R SMT Multilayer Ceramic Capacitor "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-4064-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/CC0603KRX7R7BB152/311-4064-1-ND/8025153?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="CC0603KRX7R7BB152"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1_05X2MM" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="RC0603JR-0710KL" package="RESC1607X60N" value="RC0603JR-0710KL">
<attribute name="DESCRIPTION" value=" RC Series 0603 0.1 W 10 kOhms 5% ±100 ppm/°C SMT Thick Film Chip Resistor "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-10KGRCT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/RC0603JR-0710KL/311-10KGRCT-ND/729647?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="RC0603JR-0710KL" package="RESC1607X60N" value="RC0603JR-0710KL">
<attribute name="DESCRIPTION" value=" RC Series 0603 0.1 W 10 kOhms 5% ±100 ppm/°C SMT Thick Film Chip Resistor "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-10KGRCT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/RC0603JR-0710KL/311-10KGRCT-ND/729647?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="RC0603JR-0710KL" package="RESC1607X60N" value="RC0603JR-0710KL">
<attribute name="DESCRIPTION" value=" RC Series 0603 0.1 W 10 kOhms 5% ±100 ppm/°C SMT Thick Film Chip Resistor "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="311-10KGRCT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/yageo/RC0603JR-0710KL/311-10KGRCT-ND/729647?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Yageo"/>
<attribute name="MP" value="RC0603JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Yageo"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="DRV5053PAQDBZR" package="SOT95P237X112-3N" value="DRV5053PAQDBZR">
<attribute name="DESCRIPTION" value=" 2.5 to 38 V Analog Bipolar Hall Effect Sensor 3-SOT-23 -40 to 125 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="296-38458-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/texas-instruments/DRV5053PAQDBZR/296-38458-1-ND/5022223?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="DRV5053PAQDBZR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3 Texas Instruments"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="DRV5053PAQDBZR" package="SOT95P237X112-3N" value="DRV5053PAQDBZR">
<attribute name="DESCRIPTION" value=" 2.5 to 38 V Analog Bipolar Hall Effect Sensor 3-SOT-23 -40 to 125 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="296-38458-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/texas-instruments/DRV5053PAQDBZR/296-38458-1-ND/5022223?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="DRV5053PAQDBZR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3 Texas Instruments"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="DRV5053PAQDBZR" package="SOT95P237X112-3N" value="DRV5053PAQDBZR">
<attribute name="DESCRIPTION" value=" 2.5 to 38 V Analog Bipolar Hall Effect Sensor 3-SOT-23 -40 to 125 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="296-38458-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/texas-instruments/DRV5053PAQDBZR/296-38458-1-ND/5022223?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="DRV5053PAQDBZR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-3 Texas Instruments"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
