(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector_Generic:Conn_01x04" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0))
      (property "Value" "Conn_01x04" (id 1) (at 0 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x04_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 1.27 -6.35)
          (fill (type background))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "MKRWAN:ABX00012" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -25.4 21.082 0))
      (property "Value" "ABX00012" (id 1) (at -25.4 -22.86 0))
      (property "Footprint" "ARDUINO_ABX00012" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "" (id 4) (at 0 0 0))
      (property "MANUFACTURER" "Arduino" (id 5) (at 0 0 0))
      (property "PARTREV" "5" (id 6) (at 0 0 0))
      (property "STANDARD" "Manufacturer Recommendations" (id 7) (at 0 0 0))
      (symbol "ABX00012_0_0"
        (rectangle (start -25.4 -20.32) (end 25.4 20.32)
          (fill (type background))
        )
        (pin bidirectional line (at -30.48 15.24 0) (length 5.08)
          (name "PA03_VREFA/AREF")
          (number "1")
        )
        (pin bidirectional line (at -30.48 -7.62 0) (length 5.08)
          (name "PA23_TC4-W1/1")
          (number "10")
        )
        (pin bidirectional line (at -30.48 -10.16 0) (length 5.08)
          (name "PA10_TCC0-W2/~2")
          (number "11")
        )
        (pin bidirectional line (at -30.48 -12.7 0) (length 5.08)
          (name "PA11_TCC0-W3/~3")
          (number "12")
        )
        (pin bidirectional line (at -30.48 -15.24 0) (length 5.08)
          (name "PB10_TCC0-W4/~4")
          (number "13")
        )
        (pin bidirectional line (at -30.48 -17.78 0) (length 5.08)
          (name "PB11_TCC0-W5/~5")
          (number "14")
        )
        (pin bidirectional line (at 30.48 -17.78 180) (length 5.08)
          (name "PA20_TCC0-W6")
          (number "15")
        )
        (pin bidirectional line (at 30.48 -15.24 180) (length 5.08)
          (name "PA21_TCC0-W7")
          (number "16")
        )
        (pin bidirectional line (at 30.48 -12.7 180) (length 5.08)
          (name "PA16_S1_MOSI")
          (number "17")
        )
        (pin bidirectional line (at 30.48 -10.16 180) (length 5.08)
          (name "PA17_S1_SCK")
          (number "18")
        )
        (pin bidirectional line (at 30.48 -7.62 180) (length 5.08)
          (name "PA19_S1_MISO")
          (number "19")
        )
        (pin bidirectional line (at -30.48 12.7 0) (length 5.08)
          (name "PA02_AIN0/DAC0/A0")
          (number "2")
        )
        (pin bidirectional line (at 30.48 -5.08 180) (length 5.08)
          (name "PA08_S0_I2C_SDA")
          (number "20")
        )
        (pin bidirectional line (at 30.48 -2.54 180) (length 5.08)
          (name "PA09_S0_I2C_SCL")
          (number "21")
        )
        (pin bidirectional line (at 30.48 0 180) (length 5.08)
          (name "PB23_S5_RX")
          (number "22")
        )
        (pin bidirectional line (at 30.48 2.54 180) (length 5.08)
          (name "PB22_S5_TX")
          (number "23")
        )
        (pin input line (at 30.48 5.08 180) (length 5.08)
          (name "RESET")
          (number "24")
        )
        (pin power_in line (at 30.48 7.62 180) (length 5.08)
          (name "GND")
          (number "25")
        )
        (pin power_in line (at 30.48 10.16 180) (length 5.08)
          (name "+3V3")
          (number "26")
        )
        (pin power_in line (at 30.48 12.7 180) (length 5.08)
          (name "VIN")
          (number "27")
        )
        (pin power_in line (at 30.48 15.24 180) (length 5.08)
          (name "+5V")
          (number "28")
        )
        (pin bidirectional line (at -30.48 10.16 0) (length 5.08)
          (name "PB02_AIN10/A1")
          (number "3")
        )
        (pin bidirectional line (at -30.48 7.62 0) (length 5.08)
          (name "PB03_AIN11/A2")
          (number "4")
        )
        (pin bidirectional line (at -30.48 5.08 0) (length 5.08)
          (name "PA04_AIN4/A3")
          (number "5")
        )
        (pin bidirectional line (at -30.48 2.54 0) (length 5.08)
          (name "PA05_AIN5/A4")
          (number "6")
        )
        (pin bidirectional line (at -30.48 0 0) (length 5.08)
          (name "PA06_AIN6/A5")
          (number "7")
        )
        (pin bidirectional line (at -30.48 -2.54 0) (length 5.08)
          (name "PA07_AIN7/A6")
          (number "8")
        )
        (pin bidirectional line (at -30.48 -5.08 0) (length 5.08)
          (name "PA22_TC4-W0/0")
          (number "9")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 196.85 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 191.77 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 191.77 59.69) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 128.27 125.73) (xy 130.81 125.73)))
  (wire (pts (xy 120.65 59.69) (xy 125.73 59.69)))
  (wire (pts (xy 196.85 129.54) (xy 196.85 135.89)))
  (wire (pts (xy 260.35 60.96) (xy 265.43 60.96)))
  (wire (pts (xy 265.43 58.42) (xy 260.35 58.42)))
  (wire (pts (xy 121.92 69.85) (xy 125.73 69.85)))
  (wire (pts (xy 121.92 62.23) (xy 125.73 62.23)))
  (wire (pts (xy 186.69 62.23) (xy 191.77 62.23)))
  (wire (pts (xy 186.69 74.93) (xy 190.5 74.93)))
  (wire (pts (xy 191.77 59.69) (xy 191.77 62.23)))
  (wire (pts (xy 260.35 128.27) (xy 264.16 128.27)))
  (wire (pts (xy 63.5 59.69) (xy 68.58 59.69)))
  (wire (pts (xy 121.92 72.39) (xy 125.73 72.39)))
  (wire (pts (xy 261.62 97.79) (xy 265.43 97.79)))
  (wire (pts (xy 260.35 82.55) (xy 265.43 82.55)))
  (wire (pts (xy 261.62 95.25) (xy 265.43 95.25)))
  (wire (pts (xy 121.92 74.93) (xy 125.73 74.93)))
  (wire (pts (xy 191.77 64.77) (xy 194.31 64.77)))
  (wire (pts (xy 261.62 102.87) (xy 265.43 102.87)))
  (wire (pts (xy 191.77 57.15) (xy 191.77 59.69)))
  (wire (pts (xy 191.77 59.69) (xy 194.31 59.69)))
  (wire (pts (xy 261.62 100.33) (xy 265.43 100.33)))
  (wire (pts (xy 62.23 83.82) (xy 67.31 83.82)))
  (wire (pts (xy 265.43 55.88) (xy 260.35 55.88)))
  (wire (pts (xy 63.5 62.23) (xy 68.58 62.23)))
  (wire (pts (xy 127 128.27) (xy 130.81 128.27)))
  (wire (pts (xy 186.69 64.77) (xy 191.77 64.77)))
  (wire (pts (xy 265.43 80.01) (xy 260.35 80.01)))
  (wire (pts (xy 62.23 81.28) (xy 67.31 81.28)))
  (wire (pts (xy 186.69 77.47) (xy 190.5 77.47)))
  (wire (pts (xy 121.92 67.31) (xy 125.73 67.31)))
  (wire (pts (xy 127 133.35) (xy 130.81 133.35)))
  (wire (pts (xy 261.62 120.65) (xy 264.16 120.65)))
  (wire (pts (xy 127 130.81) (xy 130.81 130.81)))
  (wire (pts (xy 62.23 78.74) (xy 67.31 78.74)))
  (wire (pts (xy 63.5 57.15) (xy 68.58 57.15)))
  (wire (pts (xy 191.77 64.77) (xy 191.77 67.31)))
  (wire (pts (xy 265.43 77.47) (xy 260.35 77.47)))
  (global_label "3.3" (shape input) (at 68.58 59.69 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 74.0169 59.6106 0))
  )
  (global_label " V.Battery" (shape input) (at 204.47 129.54 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 216.2569 129.6194 0))
  )
  (global_label "SCL" (shape input) (at 127 130.81 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 121.0793 130.8894 0))
  )
  (global_label "3.3" (shape input) (at 260.35 80.01 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 254.9131 80.0894 0))
  )
  (global_label "3.3" (shape input) (at 260.35 58.42 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 254.9131 58.4994 0))
  )
  (global_label "Value B" (shape input) (at 120.65 59.69 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 110.8588 59.6106 0))
  )
  (global_label "3.3" (shape input) (at 261.62 97.79 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 256.1831 97.8694 0))
  )
  (global_label "3.3" (shape input) (at 194.31 59.69 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 199.7469 59.6106 0))
  )
  (global_label "GND" (shape input) (at 261.62 95.25 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 255.3364 95.3294 0))
  )
  (global_label "GND" (shape input) (at 260.35 55.88 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 254.0664 55.9594 0))
  )
  (global_label "SCK" (shape input) (at 121.92 74.93 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 115.7574 74.8506 0))
  )
  (global_label "DOUT" (shape input) (at 121.92 72.39 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 114.6083 72.3106 0))
  )
  (global_label "GND" (shape input) (at 194.31 64.77 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 200.5936 64.6906 0))
  )
  (global_label "DHT22_Val1" (shape input) (at 68.58 57.15 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 82.0602 57.2294 0))
  )
  (global_label "SDA" (shape input) (at 190.5 77.47 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 196.4812 77.3906 0))
  )
  (global_label "Temp_Val" (shape input) (at 260.35 82.55 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 249.1679 82.4706 0))
  )
  (global_label "GND" (shape input) (at 67.31 83.82 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 73.5936 83.7406 0))
  )
  (global_label "GND" (shape input) (at 128.27 125.73 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 121.9864 125.8094 0))
  )
  (global_label "3.3" (shape input) (at 67.31 81.28 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 72.7469 81.2006 0))
  )
  (global_label "Temp_Val" (shape input) (at 260.35 60.96 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 249.1679 60.8806 0))
  )
  (global_label " V.Battery" (shape input) (at 260.35 128.27 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 248.5631 128.1906 0))
  )
  (global_label "DOUT" (shape input) (at 261.62 100.33 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 254.3083 100.2506 0))
  )
  (global_label "Temp_Val" (shape input) (at 121.92 62.23 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 110.7379 62.1506 0))
  )
  (global_label "Value B" (shape input) (at 196.85 135.89 270) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 196.7706 145.6812 90))
  )
  (global_label "DHT22_Val1" (shape input) (at 121.92 67.31 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 108.4398 67.2306 0))
  )
  (global_label "DHT22_Val2" (shape input) (at 67.31 78.74 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 80.7902 78.8194 0))
  )
  (global_label "GND" (shape input) (at 189.23 129.54 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 182.9464 129.4606 0))
  )
  (global_label "GND" (shape input) (at 260.35 77.47 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 254.0664 77.5494 0))
  )
  (global_label "SCL" (shape input) (at 190.5 74.93 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 196.4207 74.8506 0))
  )
  (global_label "SCK" (shape input) (at 261.62 102.87 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 255.4574 102.7906 0))
  )
  (global_label "SDA" (shape input) (at 127 133.35 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 121.0188 133.4294 0))
  )
  (global_label "GND" (shape input) (at 68.58 62.23 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 74.8636 62.1506 0))
  )
  (global_label "GND" (shape input) (at 261.62 120.65 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 255.3364 120.7294 0))
  )
  (global_label "3.3" (shape input) (at 127 128.27 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 121.5631 128.3494 0))
  )
  (global_label "DHT22_Val2" (shape input) (at 121.92 69.85 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 108.4398 69.7706 0))
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 269.24 123.19 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J4" (id 0) (at 271.78 123.1899 0))
    (property "Value" "Battery Reader" (id 1) (at 271.78 125.7299 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 269.24 123.19 0))
    (property "Datasheet" "~" (id 3) (at 269.24 123.19 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "power:+3V3") (at 191.77 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0101" (id 0) (at 191.77 60.96 0))
    (property "Value" "+3V3" (id 1) (at 191.77 52.07 0))
    (property "Footprint" "" (id 2) (at 191.77 57.15 0))
    (property "Datasheet" "" (id 3) (at 191.77 57.15 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 135.89 128.27 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J3" (id 0) (at 138.43 128.2699 0))
    (property "Value" "Gravity WattMeter" (id 1) (at 138.43 130.8099 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 135.89 128.27 0))
    (property "Datasheet" "~" (id 3) (at 135.89 128.27 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 58.42 59.69 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J2" (id 0) (at 58.42 48.26 0))
    (property "Value" "DHT22" (id 1) (at 58.42 50.8 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 58.42 59.69 0))
    (property "Datasheet" "~" (id 3) (at 58.42 59.69 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:R") (at 200.66 129.54 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 200.66 123.19 90))
    (property "Value" "100 Ohm" (id 1) (at 200.66 125.73 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (id 2) (at 200.66 127.762 90))
    (property "Datasheet" "~" (id 3) (at 200.66 129.54 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MKRWAN:ABX00012") (at 156.21 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 156.21 46.99 0))
    (property "Value" "MKR WAN" (id 1) (at 156.21 49.53 0))
    (property "Footprint" "MKR WAN:MKR WAN" (id 2) (at 156.21 72.39 0))
    (property "Datasheet" "" (id 3) (at 156.21 72.39 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "" (id 4) (at 156.21 72.39 0))
    (property "MANUFACTURER" "Arduino" (id 5) (at 156.21 72.39 0))
    (property "PARTREV" "5" (id 6) (at 156.21 72.39 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 7) (at 156.21 72.39 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 270.51 58.42 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J5" (id 0) (at 273.05 58.4199 0))
    (property "Value" "Temp1" (id 1) (at 273.05 60.9599 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 270.51 58.42 0))
    (property "Datasheet" "~" (id 3) (at 270.51 58.42 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 270.51 97.79 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J7" (id 0) (at 273.05 97.7899 0))
    (property "Value" "HX711" (id 1) (at 273.05 100.33 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 270.51 97.79 0))
    (property "Datasheet" "~" (id 3) (at 270.51 97.79 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:R") (at 193.04 129.54 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R1" (id 0) (at 193.04 123.19 90))
    (property "Value" "100 Ohm" (id 1) (at 193.04 125.73 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (id 2) (at 193.04 127.762 90))
    (property "Datasheet" "~" (id 3) (at 193.04 129.54 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 57.15 81.28 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 57.15 69.85 0))
    (property "Value" "DHT22" (id 1) (at 57.15 72.39 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 57.15 81.28 0))
    (property "Datasheet" "~" (id 3) (at 57.15 81.28 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "power:GND") (at 191.77 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0102" (id 0) (at 191.77 73.66 0))
    (property "Value" "GND" (id 1) (at 191.77 72.39 0))
    (property "Footprint" "" (id 2) (at 191.77 67.31 0))
    (property "Datasheet" "" (id 3) (at 191.77 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 270.51 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J6" (id 0) (at 273.05 80.0099 0))
    (property "Value" "Temp2" (id 1) (at 273.05 82.5499 0))
    (property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (id 2) (at 270.51 80.01 0))
    (property "Datasheet" "~" (id 3) (at 270.51 80.01 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR0101") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "J1") (unit 1) (value "DHT22") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J2") (unit 1) (value "DHT22") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J3") (unit 1) (value "Gravity WattMeter") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J4") (unit 1) (value "Battery Reader") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J5") (unit 1) (value "Temp1") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J6") (unit 1) (value "Temp2") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "J7") (unit 1) (value "HX711") (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical")
    )
    (path
      (reference "R1") (unit 1) (value "100 Ohm") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
    )
    (path
      (reference "R2") (unit 1) (value "100 Ohm") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal")
    )
    (path
      (reference "U1") (unit 1) (value "MKR WAN") (footprint "MKR WAN:MKR WAN")
    )
  )
)
