(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Node 3/4")
    (date "22.11.2023")
    (rev "0")
    (company "Lyubomir Nachev")
  )
  (lib_symbols
    (symbol "BME688:BME688" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 6.35 2.54 0))
      (property "Value" "BME688" (id 1) (at -1.27 2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "BME688_0_1"
        (rectangle (start -6.35 1.27) (end 8.89 -10.16)
          (fill (type background))
        )
      )
      (symbol "BME688_1_1"
        (pin power_in line (at -3.81 -12.7 90) (length 2.54)
          (name "2-6V")
          (number "1")
        )
        (pin bidirectional line (at -1.27 -12.7 90) (length 2.54)
          (name "SDA")
          (number "2")
        )
        (pin bidirectional line (at 1.27 -12.7 90) (length 2.54)
          (name "SCL")
          (number "3")
        )
        (pin no_connect line (at 3.81 -12.7 90) (length 2.54)
          (name "N/C")
          (number "4")
        )
        (pin power_in line (at 6.35 -12.7 90) (length 2.54)
          (name "GND")
          (number "5")
        )
      )
    )
    (symbol "BU30TD3WG:BU30TD3WG" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 10.16 -1.27 0))
      (property "Value" "BU30TD3WG" (id 1) (at -1.27 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "BU30TD3WG_0_0"
        (pin power_in line (at -11.43 -5.08 0) (length 5.08)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at -11.43 -7.62 0) (length 5.08)
          (name "GND")
          (number "2")
        )
        (pin input line (at -11.43 -10.16 0) (length 5.08)
          (name "STBY")
          (number "3")
        )
        (pin no_connect line (at 16.51 -5.08 180) (length 5.08)
          (name "N.C.")
          (number "4")
        )
        (pin output line (at 16.51 -7.62 180) (length 5.08)
          (name "VOUT")
          (number "5")
        )
      )
      (symbol "BU30TD3WG_0_1"
        (polyline
          (pts
            (xy -6.35 -2.54)
            (xy 11.43 -2.54)
            (xy 11.43 -12.7)
            (xy -6.35 -12.7)
            (xy -6.35 -2.54)
          )
          (fill (type background))
        )
      )
    )
    (symbol "Device:Battery_Cell" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (id 0) (at 2.54 2.54 0))
      (property "Value" "Battery_Cell" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 1.524 90))
      (property "Datasheet" "~" (id 3) (at 0 1.524 90))
      (property "ki_keywords" "battery cell" (id 4) (at 0 0 0))
      (property "ki_description" "Single-cell battery" (id 5) (at 0 0 0))
      (symbol "Battery_Cell_0_1"
        (rectangle (start -2.286 1.778) (end 2.286 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.5748 1.1938) (end 1.4732 0.6858)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 3.429)
            (xy 1.524 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 3.937)
            (xy 1.016 2.921)
          )
          (fill (type none))
        )
      )
      (symbol "Battery_Cell_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:Buzzer" (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BZ" (id 0) (at 3.81 1.27 0))
      (property "Value" "Buzzer" (id 1) (at 3.81 -1.27 0))
      (property "Footprint" "" (id 2) (at -0.635 2.54 90))
      (property "Datasheet" "~" (id 3) (at -0.635 2.54 90))
      (property "ki_keywords" "quartz resonator ceramic" (id 4) (at 0 0 0))
      (property "ki_description" "Buzzer, polarized" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "*Buzzer*" (id 6) (at 0 0 0))
      (symbol "Buzzer_0_1"
        (arc (start 0 -3.175) (mid 3.175 0) (end 0 3.175)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.651 1.905)
            (xy -1.143 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.397 2.159)
            (xy -1.397 1.651)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 3.175)
            (xy 0 -3.175)
          )
          (fill (type none))
        )
      )
      (symbol "Buzzer_1_1"
        (pin passive line (at -2.54 2.54 0) (length 2.54)
          (name "-")
          (number "1")
        )
        (pin passive line (at -2.54 -2.54 0) (length 2.54)
          (name "+")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:1N5817" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "1N5817" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "20V 1A Schottky Barrier Rectifier Diode, DO-41" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (id 6) (at 0 0 0))
      (symbol "1N5817_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "1N5817_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Mechanical:MountingHole" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 5.08 0))
      (property "Value" "MountingHole" (id 1) (at 0 3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0))
      (property "ki_description" "Mounting Hole without connection" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "MountingHole*" (id 6) (at 0 0 0))
      (symbol "MountingHole_0_1"
        (circle (center 0 0) (radius 1.27)
          (fill (type none))
        )
      )
    )
    (symbol "NRF52840-DONGLE:NRF52840-DONGLE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U5" (id 0) (at 8.89 21.59 0))
      (property "Value" "NRF52840-DONGLE" (id 1) (at 10.16 -19.05 0))
      (property "Footprint" "custom:MODULE_NRF52840-DONGLE" (id 2) (at 0 -22.86 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "PARTREV" "1.1" (id 4) (at 0 -5.08 0))
      (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 5.08 -25.4 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "N/A" (id 6) (at 0 -2.54 0))
      (property "MANUFACTURER" "Nordic semiconductor" (id 7) (at -1.27 -20.32 0))
      (symbol "NRF52840-DONGLE_0_0"
        (rectangle (start -10.16 20.32) (end 10.16 -17.78)
          (fill (type background))
        )
        (pin bidirectional line (at -15.24 12.7 0) (length 5.08)
          (name "SWDIO")
          (number "1")
        )
        (pin bidirectional line (at -15.24 -12.7 0) (length 5.08)
          (name "0.10")
          (number "10")
        )
        (pin power_in line (at 15.24 -10.16 180) (length 5.08)
          (name "GND")
          (number "11")
        )
        (pin input clock (at -15.24 15.24 0) (length 5.08)
          (name "SWDCLK")
          (number "12")
        )
        (pin power_in line (at 15.24 17.78 180) (length 5.08)
          (name "VBUS")
          (number "13")
        )
        (pin output line (at 15.24 12.7 180) (length 5.08)
          (name "OUT")
          (number "14")
        )
        (pin power_in line (at 15.24 -12.7 180) (length 5.08)
          (name "GND")
          (number "15")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 5.08)
          (name "0.31")
          (number "16")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 5.08)
          (name "0.29")
          (number "17")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 5.08)
          (name "0.02")
          (number "18")
        )
        (pin bidirectional line (at 15.24 0 180) (length 5.08)
          (name "1.15")
          (number "19")
        )
        (pin bidirectional line (at -15.24 7.62 0) (length 5.08)
          (name "0.13")
          (number "2")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 5.08)
          (name "1.13")
          (number "20")
        )
        (pin bidirectional line (at 15.24 -5.08 180) (length 5.08)
          (name "1.10")
          (number "21")
        )
        (pin power_in line (at 15.24 -15.24 180) (length 5.08)
          (name "GND")
          (number "22")
        )
        (pin bidirectional line (at -15.24 5.08 0) (length 5.08)
          (name "0.15")
          (number "3")
        )
        (pin bidirectional line (at -15.24 2.54 0) (length 5.08)
          (name "0.17")
          (number "4")
        )
        (pin bidirectional line (at -15.24 0 0) (length 5.08)
          (name "0.20")
          (number "5")
        )
        (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
          (name "0.22")
          (number "6")
        )
        (pin bidirectional line (at -15.24 -5.08 0) (length 5.08)
          (name "0.24")
          (number "7")
        )
        (pin bidirectional line (at -15.24 -7.62 0) (length 5.08)
          (name "1.00")
          (number "8")
        )
        (pin bidirectional line (at -15.24 -10.16 0) (length 5.08)
          (name "0.09")
          (number "9")
        )
      )
    )
    (symbol "TP4056_module:TP4056" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 8.89 0 0))
      (property "Value" "TP4056" (id 1) (at -2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "TP4056_0_1"
        (rectangle (start -6.35 -1.27) (end 10.16 -11.43)
          (fill (type background))
        )
      )
      (symbol "TP4056_1_1"
        (pin power_in line (at -8.89 -2.54 0) (length 2.54)
          (name "IN+")
          (number "1")
        )
        (pin power_in line (at -8.89 -10.16 0) (length 2.54)
          (name "IN-")
          (number "2")
        )
        (pin power_out line (at 12.7 -2.54 180) (length 2.54)
          (name "OUT+")
          (number "3")
        )
        (pin power_in line (at 12.7 -5.08 180) (length 2.54)
          (name "B+")
          (number "4")
        )
        (pin power_in line (at 12.7 -7.62 180) (length 2.54)
          (name "B-")
          (number "5")
        )
        (pin power_out line (at 12.7 -10.16 180) (length 2.54)
          (name "OUT-")
          (number "6")
        )
      )
    )
    (symbol "Transistor_BJT:PN2222A" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "PN2222A" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF" (id 3) (at 0 0 0))
      (property "ki_keywords" "NPN Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?92*" (id 6) (at 0 0 0))
      (symbol "PN2222A_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0.635 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 0.635 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 0.635 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.413 -2.413)
            (xy 1.905 -1.905)
            (xy 1.905 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 -1.651)
            (xy 1.651 -1.143)
            (xy 2.159 -2.159)
            (xy 1.143 -1.651)
            (xy 1.143 -1.651)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "PN2222A_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 5.08)
          (name "B")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "power:+3V0" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V0" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V0\"" (id 5) (at 0 0 0))
      (symbol "+3V0_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V0_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V0")
          (number "1")
        )
      )
    )
    (symbol "power:GNDD" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GNDD" (id 1) (at 0 -3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GNDD\" , digital ground" (id 5) (at 0 0 0))
      (symbol "GNDD_0_1"
        (rectangle (start -1.27 -1.524) (end 1.27 -2.032)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "GNDD_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GNDD")
          (number "1")
        )
      )
    )
    (symbol "power:VBUS" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VBUS" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VBUS\"" (id 5) (at 0 0 0))
      (symbol "VBUS_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VBUS_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VBUS")
          (number "1")
        )
      )
    )
    (symbol "power:VCC" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VCC" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VCC\"" (id 5) (at 0 0 0))
      (symbol "VCC_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VCC_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VCC")
          (number "1")
        )
      )
    )
  )
  (junction (at 96.52 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 165.1 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 199.39 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 81.28) (diameter 0) (color 0 0 0 0))
  (no_connect (at 133.35 76.2))
  (no_connect (at 163.83 86.36))
  (no_connect (at 133.35 91.44))
  (no_connect (at 163.83 93.98))
  (no_connect (at 163.83 91.44))
  (no_connect (at 133.35 93.98))
  (no_connect (at 133.35 88.9))
  (no_connect (at 163.83 83.82))
  (no_connect (at 163.83 88.9))
  (no_connect (at 133.35 101.6))
  (no_connect (at 133.35 96.52))
  (no_connect (at 163.83 81.28))
  (no_connect (at 133.35 99.06))
  (no_connect (at 133.35 73.66))
  (wire (pts (xy 64.77 96.52) (xy 63.5 96.52)))
  (wire (pts (xy 198.12 104.14) (xy 191.77 104.14)))
  (wire (pts (xy 198.12 114.3) (xy 191.77 114.3)))
  (wire (pts (xy 85.09 67.31) (xy 85.09 69.85)))
  (wire (pts (xy 53.34 101.6) (xy 53.34 96.52)))
  (wire (pts (xy 209.55 76.2) (xy 207.01 76.2)))
  (wire (pts (xy 228.6 58.42) (xy 228.6 60.96)))
  (wire (pts (xy 165.1 104.14) (xy 163.83 104.14)))
  (wire (pts (xy 226.06 76.2) (xy 217.17 76.2)))
  (wire (pts (xy 165.1 106.68) (xy 165.1 104.14)))
  (wire (pts (xy 191.77 114.3) (xy 191.77 115.57)))
  (wire (pts (xy 52.07 57.15) (xy 52.07 59.69)))
  (wire (pts (xy 123.19 83.82) (xy 114.3 83.82)))
  (wire (pts (xy 123.19 83.82) (xy 133.35 83.82)))
  (wire (pts (xy 53.34 93.98) (xy 53.34 96.52)))
  (wire (pts (xy 186.69 62.23) (xy 194.31 62.23)))
  (wire (pts (xy 123.19 68.58) (xy 123.19 69.85)))
  (wire (pts (xy 97.79 67.31) (xy 97.79 69.85)))
  (wire (pts (xy 165.1 99.06) (xy 165.1 101.6)))
  (wire (pts (xy 199.39 60.96) (xy 208.28 60.96)))
  (wire (pts (xy 194.31 60.96) (xy 194.31 62.23)))
  (wire (pts (xy 96.52 101.6) (xy 96.52 99.06)))
  (wire (pts (xy 85.09 57.15) (xy 85.09 59.69)))
  (wire (pts (xy 91.44 57.15) (xy 97.79 57.15)))
  (wire (pts (xy 119.38 81.28) (xy 133.35 81.28)))
  (wire (pts (xy 83.82 67.31) (xy 85.09 67.31)))
  (wire (pts (xy 64.77 99.06) (xy 60.96 99.06)))
  (wire (pts (xy 166.37 71.12) (xy 163.83 71.12)))
  (wire (pts (xy 191.77 104.14) (xy 191.77 102.87)))
  (wire (pts (xy 123.19 78.74) (xy 123.19 83.82)))
  (wire (pts (xy 96.52 93.98) (xy 96.52 99.06)))
  (wire (pts (xy 215.9 60.96) (xy 217.17 60.96)))
  (wire (pts (xy 96.52 110.49) (xy 96.52 109.22)))
  (wire (pts (xy 52.07 59.69) (xy 53.34 59.69)))
  (wire (pts (xy 119.38 71.12) (xy 119.38 69.85)))
  (wire (pts (xy 191.77 106.68) (xy 198.12 106.68)))
  (wire (pts (xy 97.79 57.15) (xy 97.79 59.69)))
  (wire (pts (xy 96.52 99.06) (xy 92.71 99.06)))
  (wire (pts (xy 85.09 59.69) (xy 83.82 59.69)))
  (wire (pts (xy 172.72 68.58) (xy 172.72 76.2)))
  (wire (pts (xy 224.79 60.96) (xy 228.6 60.96)))
  (wire (pts (xy 60.96 59.69) (xy 62.23 59.69)))
  (wire (pts (xy 199.39 60.96) (xy 199.39 71.12)))
  (wire (pts (xy 60.96 67.31) (xy 60.96 69.85)))
  (wire (pts (xy 114.3 86.36) (xy 133.35 86.36)))
  (wire (pts (xy 191.77 109.22) (xy 198.12 109.22)))
  (wire (pts (xy 165.1 101.6) (xy 165.1 104.14)))
  (wire (pts (xy 172.72 76.2) (xy 163.83 76.2)))
  (wire (pts (xy 199.39 81.28) (xy 199.39 85.09)))
  (wire (pts (xy 64.77 101.6) (xy 63.5 101.6)))
  (wire (pts (xy 186.69 58.42) (xy 186.69 62.23)))
  (wire (pts (xy 119.38 78.74) (xy 119.38 81.28)))
  (wire (pts (xy 91.44 69.85) (xy 97.79 69.85)))
  (wire (pts (xy 163.83 99.06) (xy 165.1 99.06)))
  (wire (pts (xy 119.38 69.85) (xy 123.19 69.85)))
  (wire (pts (xy 60.96 99.06) (xy 60.96 110.49)))
  (wire (pts (xy 123.19 69.85) (xy 123.19 71.12)))
  (wire (pts (xy 91.44 62.23) (xy 91.44 57.15)))
  (wire (pts (xy 83.82 64.77) (xy 91.44 64.77)))
  (wire (pts (xy 163.83 101.6) (xy 165.1 101.6)))
  (wire (pts (xy 83.82 62.23) (xy 91.44 62.23)))
  (wire (pts (xy 91.44 64.77) (xy 91.44 69.85)))
  (wire (pts (xy 166.37 68.58) (xy 166.37 71.12)))
  (wire (pts (xy 53.34 109.22) (xy 53.34 110.49)))
  (wire (pts (xy 114.3 81.28) (xy 119.38 81.28)))
  (wire (pts (xy 60.96 67.31) (xy 62.23 67.31)))
  (wire (pts (xy 53.34 96.52) (xy 63.5 96.52)))
  (wire (pts (xy 63.5 101.6) (xy 63.5 96.52)))
  (label "SCL" (at 114.3 83.82 0))
  (label "B_PIN" (at 114.3 86.36 0))
  (label "SDA" (at 191.77 106.68 0))
  (label "B_PIN" (at 226.06 76.2 180))
  (label "SDA" (at 114.3 81.28 0))
  (label "SCL" (at 191.77 109.22 0))
  (symbol (lib_id "power:+3V0") (at 228.6 58.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR018" (id 0) (at 228.6 62.23 0))
    (property "Value" "+3V0" (id 1) (at 226.06 54.61 0))
    (property "Footprint" "" (id 2) (at 228.6 58.42 0))
    (property "Datasheet" "" (id 3) (at 228.6 58.42 0))
    (pin "1")
  )
  (symbol (lib_id "Device:LED") (at 212.09 60.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 210.82 57.15 0))
    (property "Value" "LED" (id 1) (at 212.09 64.77 0))
    (property "Footprint" "LED_THT:LED_D3.0mm" (id 2) (at 212.09 60.96 0))
    (property "Datasheet" "~" (id 3) (at 212.09 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 96.52 110.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR09" (id 0) (at 96.52 116.84 0))
    (property "Value" "GNDD" (id 1) (at 96.52 114.3 0))
    (property "Footprint" "" (id 2) (at 96.52 110.49 0))
    (property "Datasheet" "" (id 3) (at 96.52 110.49 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V0") (at 123.19 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR010" (id 0) (at 123.19 72.39 0))
    (property "Value" "+3V0" (id 1) (at 120.65 64.77 0))
    (property "Footprint" "" (id 2) (at 123.19 68.58 0))
    (property "Datasheet" "" (id 3) (at 123.19 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 85.09 57.15 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR06" (id 0) (at 85.09 60.96 0))
    (property "Value" "VCC" (id 1) (at 85.09 53.34 0))
    (property "Footprint" "" (id 2) (at 85.09 57.15 0))
    (property "Datasheet" "" (id 3) (at 85.09 57.15 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 53.34 110.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR03" (id 0) (at 53.34 116.84 0))
    (property "Value" "GNDD" (id 1) (at 53.34 114.3 0))
    (property "Footprint" "" (id 2) (at 53.34 110.49 0))
    (property "Datasheet" "" (id 3) (at 53.34 110.49 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Buzzer") (at 196.85 58.42 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BZ1" (id 0) (at 196.85 50.8 90))
    (property "Value" "Buzzer" (id 1) (at 199.39 53.34 90))
    (property "Footprint" "Buzzer_Beeper:Buzzer_12x9.5RM7.6" (id 2) (at 194.31 59.055 90))
    (property "Datasheet" "~" (id 3) (at 194.31 59.055 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V0") (at 186.69 58.42 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR016" (id 0) (at 186.69 62.23 0))
    (property "Value" "+3V0" (id 1) (at 184.15 54.61 0))
    (property "Footprint" "" (id 2) (at 186.69 58.42 0))
    (property "Datasheet" "" (id 3) (at 186.69 58.42 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 213.36 76.2 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 213.36 73.66 90))
    (property "Value" "200" (id 1) (at 213.36 78.74 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (id 2) (at 213.36 74.422 90))
    (property "Datasheet" "~" (id 3) (at 213.36 76.2 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 132.08 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H3" (id 0) (at 144.78 130.8099 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 133.3499 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm" (id 2) (at 142.24 132.08 0))
    (property "Datasheet" "~" (id 3) (at 142.24 132.08 0))
  )
  (symbol (lib_id "power:GNDD") (at 191.77 115.57 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR012" (id 0) (at 191.77 121.92 0))
    (property "Value" "GNDD" (id 1) (at 191.77 119.38 0))
    (property "Footprint" "" (id 2) (at 191.77 115.57 0))
    (property "Datasheet" "" (id 3) (at 191.77 115.57 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 119.38 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 115.57 73.66 0))
    (property "Value" "4.7k" (id 1) (at 113.03 76.2 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (id 2) (at 117.602 74.93 90))
    (property "Datasheet" "~" (id 3) (at 119.38 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V0") (at 172.72 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR015" (id 0) (at 172.72 72.39 0))
    (property "Value" "+3V0" (id 1) (at 170.18 64.77 0))
    (property "Footprint" "" (id 2) (at 172.72 68.58 0))
    (property "Datasheet" "" (id 3) (at 172.72 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 165.1 106.68 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR013" (id 0) (at 165.1 113.03 0))
    (property "Value" "GNDD" (id 1) (at 165.1 110.49 0))
    (property "Footprint" "" (id 2) (at 165.1 106.68 0))
    (property "Datasheet" "" (id 3) (at 165.1 106.68 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V0") (at 96.52 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR08" (id 0) (at 96.52 97.79 0))
    (property "Value" "+3V0" (id 1) (at 93.98 90.17 0))
    (property "Footprint" "" (id 2) (at 96.52 93.98 0))
    (property "Datasheet" "" (id 3) (at 96.52 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "power:VBUS") (at 166.37 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR014" (id 0) (at 166.37 72.39 0))
    (property "Value" "VBUS" (id 1) (at 166.37 64.77 0))
    (property "Footprint" "" (id 2) (at 166.37 68.58 0))
    (property "Datasheet" "" (id 3) (at 166.37 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 199.39 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR017" (id 0) (at 199.39 91.44 0))
    (property "Value" "GNDD" (id 1) (at 199.39 88.9 0))
    (property "Footprint" "" (id 2) (at 199.39 85.09 0))
    (property "Datasheet" "" (id 3) (at 199.39 85.09 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 220.98 60.96 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 220.98 58.42 90))
    (property "Value" "200" (id 1) (at 220.98 63.5 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (id 2) (at 220.98 62.738 90))
    (property "Datasheet" "~" (id 3) (at 220.98 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 127 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H2" (id 0) (at 144.78 125.7299 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 128.2699 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm" (id 2) (at 142.24 127 0))
    (property "Datasheet" "~" (id 3) (at 142.24 127 0))
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 137.16 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H4" (id 0) (at 144.78 135.8899 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 138.4299 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm" (id 2) (at 142.24 137.16 0))
    (property "Datasheet" "~" (id 3) (at 142.24 137.16 0))
  )
  (symbol (lib_id "power:GNDD") (at 85.09 69.85 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 85.09 76.2 0))
    (property "Value" "GNDD" (id 1) (at 85.09 73.66 0))
    (property "Footprint" "" (id 2) (at 85.09 69.85 0))
    (property "Datasheet" "" (id 3) (at 85.09 69.85 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 53.34 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 57.15 104.1399 0))
    (property "Value" "1u" (id 1) (at 57.15 106.6799 0))
    (property "Footprint" "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (id 2) (at 54.3052 109.22 0))
    (property "Datasheet" "~" (id 3) (at 53.34 105.41 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:PN2222A") (at 201.93 76.2 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q1" (id 0) (at 196.85 77.4701 0))
    (property "Value" "PN2222A" (id 1) (at 196.85 74.9301 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 196.85 74.295 0))
    (property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF" (id 3) (at 201.93 76.2 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+3V0") (at 191.77 102.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR011" (id 0) (at 191.77 106.68 0))
    (property "Value" "+3V0" (id 1) (at 189.23 99.06 0))
    (property "Footprint" "" (id 2) (at 191.77 102.87 0))
    (property "Datasheet" "" (id 3) (at 191.77 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 60.96 110.49 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR05" (id 0) (at 60.96 116.84 0))
    (property "Value" "GNDD" (id 1) (at 60.96 114.3 0))
    (property "Footprint" "" (id 2) (at 60.96 110.49 0))
    (property "Datasheet" "" (id 3) (at 60.96 110.49 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:1N5817") (at 57.15 59.69 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 57.15 55.88 0))
    (property "Value" "1N5817" (id 1) (at 57.15 62.23 0))
    (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 57.15 55.245 0))
    (property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf" (id 3) (at 57.15 59.69 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "TP4056_module:TP4056") (at 71.12 57.15 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 80.01 57.15 0))
    (property "Value" "TP4056" (id 1) (at 77.47 69.85 0))
    (property "Footprint" "custom:TP4056-18650" (id 2) (at 71.12 57.15 0))
    (property "Datasheet" "" (id 3) (at 71.12 57.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "BU30TD3WG:BU30TD3WG") (at 76.2 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 86.36 92.71 0))
    (property "Value" "BU30TD3WG" (id 1) (at 82.55 105.41 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 76.2 91.44 0))
    (property "Datasheet" "" (id 3) (at 76.2 91.44 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "NRF52840-DONGLE:NRF52840-DONGLE") (at 148.59 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 157.48 67.31 0))
    (property "Value" "NRF52840-DONGLE" (id 1) (at 158.75 107.95 0))
    (property "Footprint" "custom:MODULE_NRF52840-DONGLE" (id 2) (at 148.59 111.76 0))
    (property "Datasheet" "" (id 3) (at 148.59 88.9 0))
    (property "PARTREV" "1.1" (id 4) (at 148.59 93.98 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 153.67 114.3 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "N/A" (id 6) (at 148.59 91.44 0))
    (property "MANUFACTURER" "Nordic semiconductor" (id 7) (at 147.32 109.22 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:C") (at 96.52 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 100.33 104.1399 0))
    (property "Value" "1u" (id 1) (at 100.33 106.6799 0))
    (property "Footprint" "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (id 2) (at 97.4852 109.22 0))
    (property "Datasheet" "~" (id 3) (at 96.52 105.41 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 60.96 69.85 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 60.96 76.2 0))
    (property "Value" "GNDD" (id 1) (at 60.96 73.66 0))
    (property "Footprint" "" (id 2) (at 60.96 69.85 0))
    (property "Datasheet" "" (id 3) (at 60.96 69.85 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 53.34 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 53.34 97.79 0))
    (property "Value" "VCC" (id 1) (at 53.34 90.17 0))
    (property "Footprint" "" (id 2) (at 53.34 93.98 0))
    (property "Datasheet" "" (id 3) (at 53.34 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 121.92 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H1" (id 0) (at 144.78 120.6499 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 123.1899 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm" (id 2) (at 142.24 121.92 0))
    (property "Datasheet" "~" (id 3) (at 142.24 121.92 0))
  )
  (symbol (lib_id "Device:Battery_Cell") (at 97.79 64.77 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "BT1" (id 0) (at 101.6 61.4679 0))
    (property "Value" "3.7V Li-ion" (id 1) (at 101.6 64.0079 0))
    (property "Footprint" "custom:BHC-18650-1P" (id 2) (at 97.79 63.246 90))
    (property "Datasheet" "~" (id 3) (at 97.79 63.246 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VBUS") (at 52.07 57.15 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 52.07 60.96 0))
    (property "Value" "VBUS" (id 1) (at 52.07 53.34 0))
    (property "Footprint" "" (id 2) (at 52.07 57.15 0))
    (property "Datasheet" "" (id 3) (at 52.07 57.15 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 123.19 74.93 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 128.27 73.66 0))
    (property "Value" "4.7k" (id 1) (at 129.54 76.2 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (id 2) (at 124.968 74.93 90))
    (property "Datasheet" "~" (id 3) (at 123.19 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "BME688:BME688") (at 210.82 107.95 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 209.55 100.33 90))
    (property "Value" "BME688" (id 1) (at 204.47 118.11 90))
    (property "Footprint" "custom:BME688" (id 2) (at 210.82 107.95 0))
    (property "Datasheet" "" (id 3) (at 210.82 107.95 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "VBUS") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "#PWR09") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR010") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "#PWR011") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "#PWR012") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR013") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR014") (unit 1) (value "VBUS") (footprint "")
    )
    (path
      (reference "#PWR015") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "#PWR016") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "#PWR017") (unit 1) (value "GNDD") (footprint "")
    )
    (path
      (reference "#PWR018") (unit 1) (value "+3V0") (footprint "")
    )
    (path
      (reference "BT1") (unit 1) (value "3.7V Li-ion") (footprint "custom:BHC-18650-1P")
    )
    (path
      (reference "BZ1") (unit 1) (value "Buzzer") (footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6")
    )
    (path
      (reference "C1") (unit 1) (value "1u") (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm")
    )
    (path
      (reference "C2") (unit 1) (value "1u") (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm")
    )
    (path
      (reference "D1") (unit 1) (value "1N5817") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D2") (unit 1) (value "LED") (footprint "LED_THT:LED_D3.0mm")
    )
    (path
      (reference "H1") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm")
    )
    (path
      (reference "H2") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm")
    )
    (path
      (reference "H3") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm")
    )
    (path
      (reference "H4") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm")
    )
    (path
      (reference "Q1") (unit 1) (value "PN2222A") (footprint "Package_TO_SOT_THT:TO-92_Inline")
    )
    (path
      (reference "R1") (unit 1) (value "4.7k") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal")
    )
    (path
      (reference "R2") (unit 1) (value "4.7k") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal")
    )
    (path
      (reference "R3") (unit 1) (value "200") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal")
    )
    (path
      (reference "R4") (unit 1) (value "200") (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal")
    )
    (path
      (reference "U1") (unit 1) (value "TP4056") (footprint "custom:TP4056-18650")
    )
    (path
      (reference "U2") (unit 1) (value "BU30TD3WG") (footprint "Package_TO_SOT_SMD:SOT-23-5")
    )
    (path
      (reference "U3") (unit 1) (value "NRF52840-DONGLE") (footprint "custom:MODULE_NRF52840-DONGLE")
    )
    (path
      (reference "U4") (unit 1) (value "BME688") (footprint "custom:BME688")
    )
  )
)
