<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<circle x="0" y="0" radius="20.5" width="0.1524" layer="20"/>
<circle x="-9.681" y="-9.249" radius="4.5" width="0.1524" layer="20"/>
<circle x="3.23" y="-11.618" radius="4.5" width="0.1524" layer="20"/>
<circle x="13.155" y="-4.087" radius="4.5" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="TLE5012B E1000">
<packages>
<package name="SOIC127P600X175-8N-8-V">
<description>Original name &lt;b&gt;SOIC127P600X175-8N-8-V&lt;/b&gt;&lt;p&gt;

Max Component Height - 1.75mm</description>
</package>
</packages>
</library>
<library name="6220XX21121_62200421121">
<packages>
<package name="62200421121">
</package>
</packages>
</library>
<library name="XT30PW-M">
<packages>
<package name="AMASS_XT30PW-M">
</package>
</packages>
</library>
<library name="Eagle_WR-TBL Rising Cage Clamp (rev23a)">
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Terminal Blocks - WR-TBL Rising Cage Clamp &lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-08-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691214310003">
<description>&lt;b&gt;WR-TBL Serie 2143 - 3.81 mm Horiz. Entry Modular
&lt;br&gt;&lt;/b&gt;Max Height =8.5mm , Pitch 3.81mm , 2 Pins</description>
</package>
</packages>
</library>
<library name="20021321-00008C4LF">
<packages>
<package name="AMPHENOL_20021321-00008C4LF">
</package>
</packages>
</library>
<library name="Eagle_WR-PHD (rev25a)">
<description>&lt;BR&gt;Wurth Elektronik - Electromechanical Components - Connectors - Board-to-Board Connectors - WR-PHD &lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="62100421021">
<description>&lt;b&gt; WR-PHD&lt;/b&gt; &lt;BR&gt;1.27 mm SMT Dual Pin Header, H=3.80 mm, 4 Pins&lt;b&gt;</description>
</package>
</packages>
</library>
<library name="PAD_1.32">
<packages>
<package name="PAD_1.32">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TLE5012" library="TLE5012B E1000" package="SOIC127P600X175-8N-8-V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="6220XX21121_62200421121" package="62200421121" value="6220XX21121_62200421121">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/62200421121/W%25C3%25BCrth+Elektronik+Midcom/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value="                                                      Headers &amp; Wire Housings WR-PHD1.27mm Hdr 4P Dual Str Gold                                              "/>
<attribute name="MF" value="Würth Elektronik"/>
<attribute name="MP" value="62200421121"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/62200421121/W%25C3%25BCrth+Elektronik+Midcom/view-part/?ref=snap"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="XT30PW-M" package="AMASS_XT30PW-M" value="XT30PW-M">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/XT30PW-M/AMASS/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value="                                                      Socket; DC supply; XT30; male; PIN: 2; on PCBs; THT; Colour: yellow                                              "/>
<attribute name="MF" value="AMASS"/>
<attribute name="MP" value="XT30PW-M"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/XT30PW-M/AMASS/view-part/?ref=snap"/>
</element>
<element name="J4" library="Eagle_WR-TBL Rising Cage Clamp (rev23a)" package="691214310003" value="691214310003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/691214310003?ae"/>
<attribute name="IR-UL" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691214310003 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="Horizontal"/>
<attribute name="VALUE"/>
<attribute name="WIRE" value="24 to 16 (AWG) 0.205 to 1.31 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
</element>
<element name="J1" library="XT30PW-M" package="AMASS_XT30PW-M" value="XT30PW-M">
<attribute name="AVAILABILITY" value="Not in stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/XT30PW-M/AMASS/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value="                                                      Socket; DC supply; XT30; male; PIN: 2; on PCBs; THT; Colour: yellow                                              "/>
<attribute name="MF" value="AMASS"/>
<attribute name="MP" value="XT30PW-M"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/XT30PW-M/AMASS/view-part/?ref=snap"/>
</element>
<element name="J6" library="20021321-00008C4LF" package="AMPHENOL_20021321-00008C4LF" value="20021321-00008C4LF">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/20021321-00008C4LF/Amphenol/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value="                                                      FCI 20021321 Series 1.27mm 8 Way 2 Row Straight PCB Socket Smnt Receptacle | Amphenol FCI (Amphenol CS) 20021321-00008C4LF                                              "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="20021321-00008C4LF"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/20021321-00008C4LF/Amphenol/view-part/?ref=snap"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="Eagle_WR-PHD (rev25a)" package="62100421021" value="62100421021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/62100421021?ae"/>
<attribute name="GENDER" value="Pin Header"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="62100421021"/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="1.27 mm"/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="6220XX21121_62200421121" package="62200421121" value="6220XX21121_62200421121">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CHECK_PRICES" value="https://www.snapeda.com/parts/62200421121/W%25C3%25BCrth+Elektronik+Midcom/view-part/?ref=eda"/>
<attribute name="DESCRIPTION" value="                                                      Headers &amp; Wire Housings WR-PHD1.27mm Hdr 4P Dual Str Gold                                              "/>
<attribute name="MF" value="Würth Elektronik"/>
<attribute name="MP" value="62200421121"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="SNAPEDA_LINK" value="https://www.snapeda.com/parts/62200421121/W%25C3%25BCrth+Elektronik+Midcom/view-part/?ref=snap"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="PAD_1.32" package="PAD_1.32" value="PAD_1.32"/>
<element name="U$2" library="PAD_1.32" package="PAD_1.32" value="PAD_1.32"/>
<element name="U$3" library="PAD_1.32" package="PAD_1.32" value="PAD_1.32"/>
<element name="U$4" library="PAD_1.32" package="PAD_1.32" value="PAD_1.32"/>
<element name="U$5" library="PAD_1.32" package="PAD_1.32" value="PAD_1.32"/>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TLE5012" pad="7"/>
<contactref element="J3" pad="P"/>
<contactref element="J1" pad="P"/>
<contactref element="J6" pad="7"/>
<contactref element="J8" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J7" pad="4"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="VDD">
<contactref element="TLE5012" pad="6"/>
<contactref element="J6" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J7" pad="3"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="CSQ">
<contactref element="TLE5012" pad="3"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="DATA">
<contactref element="TLE5012" pad="4"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="IFA">
<contactref element="TLE5012" pad="5"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="IFB">
<contactref element="TLE5012" pad="8"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="IFC">
<contactref element="TLE5012" pad="1"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="TLE5012" pad="2"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="W">
<contactref element="U$1" pad="P$1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="V">
<contactref element="U$2" pad="P$1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="U">
<contactref element="U$3" pad="P$1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="POWER_P">
<contactref element="J3" pad="N"/>
<contactref element="J1" pad="N"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="SWDCLK">
<contactref element="J2" pad="3"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="J2" pad="4"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="CAN_P">
<contactref element="J8" pad="1"/>
<contactref element="J3" pad="CAN_L"/>
<contactref element="J1" pad="CAN_L"/>
</signal>
<signal name="CAN_N">
<contactref element="J8" pad="3"/>
<contactref element="J3" pad="CAN_H"/>
<contactref element="J1" pad="CAN_H"/>
</signal>
<signal name="HALL_A">
<contactref element="J6" pad="4"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="HALL_B">
<contactref element="J6" pad="6"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="HALL_C">
<contactref element="J6" pad="8"/>
<contactref element="SJ3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
