<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="77" y1="51.25" x2="3" y2="51.25" width="0" layer="20"/>
<wire x1="0" y1="48.25" x2="0" y2="-5.75" width="0" layer="20"/>
<wire x1="3" y1="-8.75" x2="77" y2="-8.75" width="0" layer="20"/>
<wire x1="80" y1="-5.75" x2="80" y2="48.25" width="0" layer="20"/>
<text>SCL</text>
<text>SDA</text>
<text>3V3</text>
<text>GND</text>
<text>USB5V</text>
<text>G</text>
<text>3V3</text>
<text>10</text>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>A0</text>
<text>UART</text>
<text>GND</text>
<text>3V3</text>
<text>N/A</text>
<text>0</text>
<text>GND</text>
<text>3V3</text>
<text>TX</text>
<text>RX</text>
<text>IIC</text>
<text>IIC</text>
<text>·</text>
<text>·</text>
<text>·</text>
<text>·</text>
<text>5</text>
<text>4</text>
<text>SCL</text>
<text>SDA</text>
<text>3V3</text>
<text>GND</text>
<text>·</text>
<text>·</text>
<text>5</text>
<text>4</text>
<text>6</text>
<text>7</text>
<text>·</text>
<text>D0</text>
<text>1</text>
<text>30</text>
<wire x1="0" y1="-5.75" x2="3" y2="-8.75" width="0" layer="20" curve="90"/>
<wire x1="3" y1="51.25" x2="0" y2="48.25" width="0" layer="20" curve="90"/>
<wire x1="80" y1="48.25" x2="77" y2="51.25" width="0" layer="20" curve="90"/>
<text>CHRG</text>
<text>DONE</text>
<wire x1="77" y1="-8.75" x2="80" y2="-5.75" width="0" layer="20" curve="90"/>
<hole x="76" y="-4.75" drill="3"/>
<hole x="76" y="47.25" drill="3"/>
<hole x="4" y="47.25" drill="3"/>
<hole x="4" y="-4.75" drill="3"/>
</plain>
<libraries>
<library name="Connector-new">
<packages>
<package name="H7-2.54">
</package>
<package name="HW4-2.0-90D">
</package>
</packages>
</library>
<library name="Discrete-new">
<packages>
<package name="SOD-523">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="F0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="3P-SMD-SHORT">
</package>
<package name="L0806">
<description>&lt;b&gt;datasheet:&lt;br&gt;
&lt;u&gt;http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0103LQH2MC_02.pdf</description>
</package>
<package name="L201610">
</package>
<package name="TP-D45MIL">
</package>
<package name="X2-SMD-L2.0X1.2X0.55MM">
</package>
</packages>
</library>
<library name="Discrete-small">
<packages>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="ESD-0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="IC-new">
<packages>
<package name="DFN8G-0.5-2X2MM">
</package>
<package name="SOT-23-6">
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://eagle.componentsearchengine.com&lt;/b&gt;&lt;p&gt;&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P490X110-8N">
<description>&lt;b&gt;DGK  (S-PDSO-G8)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SON50P300X300X90-9N">
<description>&lt;b&gt;DFN-8_2022&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOD3716X145N">
<description>&lt;b&gt;1N5819HW-7-F&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="AQ753808UTG">
<description>&lt;b&gt;AQ7538-08UTG-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOT65P490X110-8N">
<description>&lt;b&gt;SOT505-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="MJ13510SMTTR">
<description>&lt;b&gt;MJ1-3510-SMT-TR-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="Connectors">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Connectors&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="S2B-PH-SM4-TB(LF)(SN)">
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4078">
<description>&lt;b&gt;DC POWER JACK 2.5mm&lt;/b&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1162.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="Baltic_Expansion_board_v1.2">
<description>Generated from &lt;b&gt;Baltic_Expansion_board_v1.2.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MOUDLE-NEW_MOUDLE14P-2.54-21X17.8MM-TEST">
</package>
<package name="CONNECTOR-NEW_MICRO-SD9+4P-SMD-16.1X14.5X1.85MM">
</package>
<package name="MOUDLE-NEW_OLED30P-0.7-24.74X16.9MM">
</package>
<package name="CONNECTOR-NEW_BAT2P-SMD-13.2X12.1X3.2MM">
</package>
<package name="DISCRETE-SMALL_C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="LED">
<description>&lt;B&gt;LED parts CHIP-Flat Top, Round Top</description>
<packages>
<package name="LEDC2012X110N_FLAT-R">
<description>Chip LED, 2.00 X 1.25 X 1.10 mm body
 &lt;p&gt;Chip LED package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
</package>
<package name="LEDC2012X110N_FLAT-G">
<description>Chip LED, 2.00 X 1.25 X 1.10 mm body
 &lt;p&gt;Chip LED package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Switch">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Switches&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="KSC222JLFS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Discrete-small" package="C0402" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="Discrete-small" package="C0603" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Discrete-small" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Discrete-small" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Discrete-small" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="Discrete-small" package="C0603" value="4.7uF/10V">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Discrete-small" package="C0603" value="2.2uF/10V">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Discrete-small" package="ESD-0402" value="ESD9B3.3ST5G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Discrete-new" package="SOD-523" value="1N4148WT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Discrete-new" package="SOD-523" value="1N4148WT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="Discrete-new" package="SOD-523" value="1N4148WT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB3" library="Discrete-new" package="F0402" value="120R/2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="Connector-new" package="H7-2.54" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="Connector-new" package="H7-2.54" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Baltic_Expansion_board_v1.2" package="CONNECTOR-NEW_MICRO-SD9+4P-SMD-16.1X14.5X1.85MM" value="ST-TF-003J">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="SKU" value="320090000"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Discrete-new" package="3P-SMD-SHORT" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Discrete-new" package="L0806" value="2.2uH">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Discrete-new" package="L201610" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Discrete-small" package="R0402" value="8.06K_1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="Discrete-small" package="R0402" value="33K_1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="Discrete-small" package="R0402" value="620K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="Discrete-small" package="R0402" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="Discrete-small" package="R0402" value="100K_1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="Discrete-small" package="R0402" value="22K_1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="Discrete-small" package="R0402" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="Discrete-small" package="R0402" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="Discrete-small" package="R0402" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Discrete-small" package="R0603" value="0R">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Discrete-small" package="R0402" value="100K_1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="Discrete-small" package="R0402" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R62" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R63" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="Discrete-small" package="R0402" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="Discrete-new" package="TP-D45MIL" value="0">
<attribute name="NAME"/>
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="TP2" library="Discrete-new" package="TP-D45MIL" value="0">
<attribute name="NAME"/>
<attribute name="PARTNO" value="DNP"/>
</element>
<element name="U1" library="SamacSys_Parts" package="SOT65P490X110-8N" value="PCF8563T">
<attribute name="ARROW_PART_NUMBER" value="PCF8563TS/5,118"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/pcf8563ts5118/nxp-semiconductors?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="NXP - PCF8563TS/5,118 - REAL TIME CLOCK, 5.5V, I2C, TSSOP-8"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="NXP"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PCF8563TS/5,118"/>
<attribute name="MOUSER_PART_NUMBER" value="771-PCF8563TS/5118"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/NXP-Semiconductors/PCF8563TS-5118?qs=beN0Cyoe8Ynnzly4fQaDyw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Baltic_Expansion_board_v1.2" package="MOUDLE-NEW_MOUDLE14P-2.54-21X17.8MM-TEST" value="Seeeduino XIAO">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="X"/>
</element>
<element name="U3" library="IC-new" package="DFN8G-0.5-2X2MM" value="ETA3410">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="IC-new" package="SOT-23-6" value="ETA1038">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="Baltic_Expansion_board_v1.2" package="MOUDLE-NEW_OLED30P-0.7-24.74X16.9MM" value="SSD1315">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="Discrete-new" package="X2-SMD-L2.0X1.2X0.55MM" value="32.768khz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="Discrete-new" package="F0402" value="120R/2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Connector-new" package="HW4-2.0-90D" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Connector-new" package="HW4-2.0-90D" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="Connector-new" package="HW4-2.0-90D" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="Connector-new" package="HW4-2.0-90D" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="Baltic_Expansion_board_v1.2" package="CONNECTOR-NEW_BAT2P-SMD-13.2X12.1X3.2MM" value="CR1220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Discrete-small" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="Discrete-small" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="SOP65P490X110-8N" value="INA332AIDGKRG4">
<attribute name="ARROW_PART_NUMBER" value="INA332AIDGKRG4"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/ina332aidgkrg4/texas-instruments?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="Instrumentation Amplifiers Lo-Pwr Single Sply CMOS Low Cost"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="INA332AIDGKRG4"/>
<attribute name="MOUSER_PART_NUMBER" value="595-INA332AIDGKRG4"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/INA332AIDGKRG4?qs=VBduBm9rCJTxc0zu0wKcuw%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="Discrete-small" package="R0402" value="263">
<attribute name="VALUE"/>
</element>
<element name="R27" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="R28" library="Discrete-small" package="R0402" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="C31" library="Discrete-small" package="C0402" value="100nF">
<attribute name="VALUE"/>
</element>
<element name="C32" library="Discrete-small" package="C0402" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="R30" library="Discrete-small" package="R0402" value="100">
<attribute name="VALUE"/>
</element>
<element name="R29" library="Discrete-small" package="R0402" value="100">
<attribute name="VALUE"/>
</element>
<element name="C33" library="Discrete-small" package="C0402" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="C34" library="Discrete-small" package="C0402" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="C35" library="Discrete-small" package="C0402" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C36" library="Discrete-small" package="C0402" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="SON50P300X300X90-9N" value="CN3165">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Lithium battery charge management chip that can be powered by solar panels"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="ShangHai Consonance Elec"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CN3165"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="Connectors" package="S2B-PH-SM4-TB(LF)(SN)" value="S2B-PH-SM4-TB(LF)(SN)">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGI_KEY_PART_NUMBER" value="455-1749-1-ND"/>
<attribute name="MANUFACTURER" value="JST Sales America Inc."/>
<attribute name="MPN" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="PACKAGE" value="SMD"/>
</element>
<element name="C1" library="Baltic_Expansion_board_v1.2" package="DISCRETE-SMALL_C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Baltic_Expansion_board_v1.2" package="DISCRETE-SMALL_C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="Discrete-small" package="R0603" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-jack" package="SPC4078" value="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SamacSys_Parts" package="SOD3716X145N" value="1N5819HW-7-F">
<attribute name="ARROW_PART_NUMBER" value="1N5819HW-7-F"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/1n5819hw-7-f/diodes-incorporated?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="Diode Schottky 1A 40V SOD123 Diodes Inc 1N5819HW-7-F, SMT Schottky Diode, 40V 1A, 2-Pin SOD-123"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1N5819HW-7-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-1N5819HW-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/1N5819HW-7-F?qs=NQ47qNm99eDyWTEd07miYA%3D%3D"/>
</element>
<element name="D6" library="SamacSys_Parts" package="SOD3716X145N" value="1N5819HW-7-F">
<attribute name="ARROW_PART_NUMBER" value="1N5819HW-7-F"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/1n5819hw-7-f/diodes-incorporated?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="Diode Schottky 1A 40V SOD123 Diodes Inc 1N5819HW-7-F, SMT Schottky Diode, 40V 1A, 2-Pin SOD-123"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Incorporated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1N5819HW-7-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-1N5819HW-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/1N5819HW-7-F?qs=NQ47qNm99eDyWTEd07miYA%3D%3D"/>
</element>
<element name="D7" library="LED" package="LEDC2012X110N_FLAT-G" value="GREEN">
<attribute name="CATEGORY" value="LED"/>
<attribute name="COLOR" value="Green"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value="Green LED Indication 0805 (2012 Metric)"/>
<attribute name="FORWARD_CURRENT" value=""/>
<attribute name="FORWARD_VOLTAGE" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0805"/>
<attribute name="PACKAGE_TYPE" value="Surface Mount"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Chip LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="Square with Flat Top"/>
</element>
<element name="D8" library="LED" package="LEDC2012X110N_FLAT-R" value="RED">
<attribute name="CATEGORY" value="LED"/>
<attribute name="COLOR" value="Red"/>
<attribute name="DATASHEET" value=""/>
<attribute name="DESCRIPTION" value="Red LED Indication 0805 (2012 Metric)"/>
<attribute name="FORWARD_CURRENT" value=""/>
<attribute name="FORWARD_VOLTAGE" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMPERATURE" value=""/>
<attribute name="PACKAGE_SIZE" value="0805"/>
<attribute name="PACKAGE_TYPE" value="Surface Mount"/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUBCATEGORY" value="Chip LED"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="Square with Flat Top"/>
</element>
<element name="R3" library="Discrete-small" package="R0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="Switch" package="KSC222JLFS" value="KSC222JLFS">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PARTNO" value="CKN9195TR-ND"/>
<attribute name="MANUFACTURER" value="C&amp;K"/>
<attribute name="MPN" value="KSC222J LFS"/>
</element>
<element name="D15" library="SamacSys_Parts" package="AQ753808UTG" value="AQ7538-08UTG">
<attribute name="ARROW_PART_NUMBER" value="AQ7538-08UTG"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/aq7538-08utg/littelfuse?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes 5V 3A +30/-22kV uDFN3810-9L Diode array"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="MANUFACTURER_NAME" value="LITTELFUSE"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AQ7538-08UTG"/>
<attribute name="MOUSER_PART_NUMBER" value="576-AQ7538-08UTG"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Littelfuse/AQ7538-08UTG?qs=Li%252BoUPsLEnv5Wi1aoEmeIw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J8" library="SamacSys_Parts" package="MJ13510SMTTR" value="MJ1-3510-SMT-TR">
<attribute name="ARROW_PART_NUMBER" value="MJ1-3510-SMT-TR"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/mj1-3510-smt-tr/cui-devices?utm_currency=USD&amp;region=nac"/>
<attribute name="DESCRIPTION" value="3.5 mm, Mono, Right Angle, Surface Mount (SMT), 2 Conductors, 1 Internal Switch, Audio Jack Connector"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="MANUFACTURER_NAME" value="Same Sky"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MJ1-3510-SMT-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="490-MJ1-3510-SMT-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CUI-Devices/MJ1-3510-SMT-TR?qs=WyjlAZoYn52cJPJjZNccVg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="13"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="9"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="J11" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="J3" pad="G2"/>
<contactref element="J3" pad="G3"/>
<contactref element="J3" pad="G4"/>
<contactref element="J3" pad="G1"/>
<contactref element="C4" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="U6" pad="8"/>
<contactref element="U6" pad="10"/>
<contactref element="U6" pad="13"/>
<contactref element="C7" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U6" pad="29"/>
<contactref element="U6" pad="30"/>
<contactref element="R24" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="BAT1" pad="V-"/>
<contactref element="C18" pad="2"/>
<contactref element="J6" pad="4"/>
<contactref element="C26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="C21" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="C20" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C32" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C35" pad="1"/>
<contactref element="C34" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J12" pad="1"/>
<contactref element="J12" pad="S1"/>
<contactref element="J12" pad="S2"/>
<contactref element="K1" pad="3"/>
<contactref element="K1" pad="4"/>
<contactref element="D15" pad="3"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="A0_D0">
<contactref element="U2" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="A1_D1">
<contactref element="U2" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="K1" pad="2"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="A6_D6_TX">
<contactref element="U2" pad="7"/>
<contactref element="J10" pad="7"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="A7_D7_RX">
<contactref element="U2" pad="8"/>
<contactref element="J11" pad="7"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="5"/>
<contactref element="C15" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="C18" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="C22" pad="1"/>
<contactref element="J12" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$29">
<contactref element="U3" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R41" pad="2"/>
<contactref element="R40" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="DATA1">
<contactref element="R60" pad="1"/>
<contactref element="J3" pad="8"/>
<contactref element="D15" pad="5"/>
</signal>
<signal name="DATA2">
<contactref element="R64" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="D15" pad="1"/>
</signal>
<signal name="VDD_3V3_SD">
<contactref element="R60" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="R63" pad="2"/>
<contactref element="R62" pad="2"/>
<contactref element="R61" pad="2"/>
<contactref element="FB3" pad="2"/>
<contactref element="J3" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="D2_SD_CS">
<contactref element="R63" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="J10" pad="4"/>
<contactref element="D15" pad="9"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="D8_SD_SCK">
<contactref element="J11" pad="6"/>
<contactref element="U2" pad="9"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="D9_SD_MISO">
<contactref element="J11" pad="5"/>
<contactref element="U2" pad="10"/>
<contactref element="R43" pad="2"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="D10_SD_MOSI">
<contactref element="J11" pad="4"/>
<contactref element="U2" pad="11"/>
<contactref element="R45" pad="2"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="D4_SDA">
<contactref element="U2" pad="5"/>
<contactref element="J10" pad="5"/>
<contactref element="U1" pad="5"/>
<contactref element="U6" pad="19"/>
<contactref element="U6" pad="20"/>
<contactref element="R9" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="D5_SCL">
<contactref element="U2" pad="6"/>
<contactref element="J10" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="U6" pad="18"/>
<contactref element="R10" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U6" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U6" pad="4"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U6" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C6" pad="1"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="U6" pad="26"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U6" pad="27"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U6" pad="28"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U6" pad="6"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="IIC_ADDR">
<contactref element="U6" pad="15"/>
<contactref element="JP1" pad="MM"/>
</signal>
<signal name="N$19">
<contactref element="JP1" pad="11"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="JP1" pad="00"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="SYS_3V3">
<contactref element="U2" pad="12"/>
<contactref element="J11" pad="3"/>
<contactref element="L2" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="FB3" pad="1"/>
<contactref element="FB1" pad="1"/>
<contactref element="D4" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="J5" pad="3"/>
<contactref element="J6" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="OLED_RST">
<contactref element="R21" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D2" pad="+"/>
<contactref element="U6" pad="14"/>
</signal>
<signal name="USB_5V">
<contactref element="U2" pad="14"/>
<contactref element="J11" pad="1"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="+"/>
<contactref element="BAT1" pad="V+@2"/>
<contactref element="BAT1" pad="V+@1"/>
</signal>
<signal name="N$23">
<contactref element="C4" pad="1"/>
<contactref element="D3" pad="-"/>
<contactref element="D4" pad="-"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="INT">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="TP2" pad="T"/>
</signal>
<signal name="CLKOUT">
<contactref element="TP1" pad="T"/>
<contactref element="U1" pad="7"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VBOOST_5V">
<contactref element="R5" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="L1" pad="2"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="R6" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R6" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U4" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="VDD_3V3_OLED">
<contactref element="FB1" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="U6" pad="9"/>
<contactref element="U6" pad="11"/>
<contactref element="D2" pad="-"/>
<contactref element="R21" pad="2"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="1"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R28" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="HY+">
<contactref element="C33" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="HY-">
<contactref element="C34" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="VIN-">
<contactref element="IC1" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="IC1" pad="3"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="ADC">
<contactref element="IC1" pad="6"/>
<contactref element="C35" pad="2"/>
<contactref element="C36" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="J10" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="KEEPOUT">
</signal>
<signal name="SOLAR">
<contactref element="IC2" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="7"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="N$25">
<contactref element="IC2" pad="6"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="N$31">
<contactref element="R43" pad="1"/>
<contactref element="J3" pad="7"/>
<contactref element="D15" pad="4"/>
</signal>
<signal name="N$33">
<contactref element="R45" pad="1"/>
<contactref element="J3" pad="3"/>
<contactref element="D15" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="D15" pad="7"/>
<contactref element="R44" pad="1"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="J2" pad="3"/>
<contactref element="D5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
