{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Digikey","Sheet1","Advanced Circuits"],"read":"whole","date_system":"1900"}

{"sheet":"Digikey","index":0,"n_rows":66,"n_cols":11,"rows_kept":66}
["Index","Quantity","Digi-Key Part Number","Manufacturer Part Number","Description","Customer Reference","Unit Price USD","Extended Price USD",null,"Costs"]
[1,{"$f":"4*3","v":12},"493-14498-ND","UKL2A100KPD","CAP ELEC 10uF 100V 10% RADIAL","MRFS_C1,C3,C6,C8",0.369,{"$f":"G2*B2","v":4.428},null,{"$f":"SUM(H:H)","v":595.5555999999999},"Subtotal"]
[2,100,"490-4789-1-ND","GCM21BR72A104KA37L","CAP CER 0.1uF 100V 10% X7R 0805","MRFS_C2,C7,C9,C10,C26,C29,C35,C36,C37,C38,C42,C45,C47,C48,C49,C50,C51,C52,C53",0.055,{"$f":"G3*B3","v":5.5},null,{"$f":"J2*0.1025","v":61.044448999999986},"Tax (Est)"]
[3,{"$f":"2*3","v":6},"P5314-ND","ECA-2AM221","CAP ELEC 220uF 100V 20% RADIAL","MRFS_C4,C5",0.82,4.92,null,{"$f":"10","v":10},"Shipping"]
[4,{"$f":"1*3","v":3},"399-13172-1-ND","C0805F683K1RAC7800","CAP CER 0.068uF 100V 10% X7R 0805","MRFS_C11",0.41,1.23,null,{"$f":"SUM(J2:J4)","v":666.6000489999999},"TOTAL"]
[5,{"$f":"4*3","v":12},"493-1668-ND","UHE2A101MPD","CAP ELEC 100uF 100V 20% RADIAL","MRFS_C12,C13,C14,C16",0.415,4.9799999999999995]
[6,{"$f":"1*3","v":3},"493-1983-ND","UPW2A331MHD","CAP ELEC 330uF 100V 20% RADIAL","MRFS_C15",1.23,3.69]
[7,{"$f":"1*3","v":3},"399-5112-1-ND","C0805F474K3RACTU","CAP CER 0.47uF 25V 10% X7R 0805","MRFS_C17",0.5,1.5]
[8,{"$f":"1*3","v":3},"399-8382-1-ND","T491D336K025AT","CAP TANT 33uF 25V 10% 2917","MRFS_C18",1.57,4.71]
[9,{"$f":"10*3","v":30},"490-14467-1-ND","GRM21BR71E225KE11L","CAP CER 2.2uF 25V 10% 0805","MRFS_C19,C20,C21,C22,C23,C24,C25,C33,C44,C46",0.151,4.53]
[10,{"$f":"2*3","v":6},"478-10197-1-ND","06031A250GAT2A","CAP CER 25pF 100V 2% 0603","MRFS_C27,C28",0.7,4.199999999999999]
[11,{"$f":"1*3","v":3},"478-8719-1-ND","12061Z475MAT2A","CAP CER 4.7uF 100V 20% 1206","MRFS_C30",1.68,5.04]
[12,{"$f":"1*3","v":3},"490-1658-1-ND","GRM21BR72A223KA01L","CAP CER 0.022uF 100V 10% X7R 0805","MRFS_C31",0.23,0.6900000000000001]
[13,{"$f":"2*3","v":6},"311-1456-1-ND","CC0805KKX7R8BB105","CAP CER 1uF 25V 10% X7R 0805","MRFS_C32,C34",0.11,0.66]
[14,{"$f":"4*3","v":12},"399-1147-1-ND","C0805C102K5RACTU","CAP CER 0.001uF 50V 10% X7R 0805","MRFS_C39,C40,C41,C43",0.043,0.516]
[15,{"$f":"16*3","v":48},"754-1946-1-ND","APTD1608LSECK/J4-PF","LED OR 2mA 1.8V 0603","MRFS_D1,D2,D5,D6,D7,D8,D9,D10,D14,D23,D26,D29,D30,D31,D32,D33",0.3968,19.0464]
[16,{"$f":"2*3","v":6},"754-1949-1-ND","APTD1608LZGCK","LED GN 2mA 2.65V 0603","MRFS_D3,D12",0.68,4.08]
[17,10,"754-2032-1-ND","APHD1608LSURCK","LED RED 2mA 1.75V 0603","MRFS_D13,D15,D16",0.302,3.02]
[18,{"$f":"1*3","v":3},"754-2040-1-ND","APTD1608LQBC/D","LED BLUE 2mA 2.65V 0603","MRFS_D11",0.64,1.92]
[19,{"$f":"1*3","v":3},"SS29-E3/52TGICT-ND","SS29-E3/52T","DIODE SCHOTTKY 90V 1.5A DO214AA","MRFS_D4",0.56,1.6800000000000002]
[20,{"$f":"10*3","v":30},"497-12278-1-ND","STPS0540ZY","Diode Schottky 40V 500mA Surface Mount SOD-123","MRFS_D17,D18,D19,D20,D21,D22,D24,D25,D27,D28",0.371,11.129999999999999]
[21,{"$f":"1*3","v":3},"277-1271-ND",1714971,"CONN TERM BLOCK 2POS 9.52MM PCB","MRFS_J1",1.53,4.59]
[22,{"$f":"1*3","v":3},"BKCT2232-4-ND","CT2232-4","4MM BINDING POST - YELLOW","MRFS_J2",4.1,12.299999999999999]
[23,{"$f":"1*3","v":3},"BKCT2232-5-ND","CT2232-5","4MM BINDING POST - GREEN","MRFS_J3",4.1,12.299999999999999]
[24,{"$f":"1*3","v":3},"BKCT2232-6-ND","CT2232-6","4MM BINDING POST - BLUE","MRFS_J4",4.1,12.299999999999999]
[25,{"$f":"1*3","v":3},"3M15450-ND","2314-6121-TG","CONN HEADER 14POS 2ROW 0.100\" PITCH","MRFS_J5",1.1,3.3000000000000003]
[26,{"$f":"4*3","v":12},"A19470-ND","640456-3","CONN HEADER VERT 3POS  0.100\" PITCH","MRFS_J6,J8,J9,J10",0.148,1.7759999999999998]
[27,{"$f":"1*3","v":3},"A19471-ND","640456-5","CONN HEADER VERT 5POS  0.100\" PITCH","MRFS_J7",0.28,0.8400000000000001]
[28,{"$f":"1*3","v":3},"541-1255-1-ND","IHLP6767GZER4R7M01","FIXED IND 4.7UH 25A 5.11 mOHM","MRFS_L1",5.87,17.61]
[29,{"$f":"1*3","v":3},"SRR1210A-331MCT-ND","SRR1210A-331M","FIXED IND 330UH 1.4A 450 mOHM","MRFS_L2",1.33,3.99]
[30,{"$f":"1*3","v":3},"445-3830-1-ND","SLF10145T-220M1R9-H","FIXED IND 22UH 1.9A 59.1 mOHM","MRFS_L3",1.65,4.949999999999999]
[31,{"$f":"8*3","v":24},"296-37482-5-ND","CSD19533KCS","MOSFET N-CH 100V 100A TO220","MRFS_M1,M2,M3,M4,M5,M6,M7,M8",1.654,39.696]
[32,10,"RMCF0603JT4K70CT-ND","RMCF0603JT4K70","RES SMD 4.7K OHM 5% 1/10W 0603","MRFS_R1,R2",0.013,0.13]
[33,{"$f":"10*3","v":30},"311-1.00KHRCT-ND","RC0603FR-071KL","RES SMD 1K OHM 1% 1/10W 0603","MRFS_R17,R18,R19,R20,R21,R49,R53,R56,R59,R62",0.015,0.44999999999999996]
[34,10,"RMCF0603JT2K20CT-ND","RMCF0603JT2K20","RES SMD 2.2K OHM 5% 1/10W 0603","MRFS_R5,R16",0.013,0.13]
[35,{"$f":"1*3","v":3},"PNM0805-50KBCT-ND","PNM0805E5002BST5","RES SMD 50K OHM 0.1% 1/5W 0805","MRFS_R6",2.76,8.28]
[36,{"$f":"1*3","v":3},"P174KDBCT-ND","ERA-3AEB1743V","RES SMD 174K OHM 0.1% 1/10W 0603","MRFS_R7",0.35,1.0499999999999998]
[37,{"$f":"8*3","v":24},"YAG3638CT-ND","AC0603JR-0710RL","RES SMD 10 OHM 5% 1/10W 0603","MRFS_R8,R9,R39,R40,R41,R42,R43,R44",0.02,0.48]
[38,{"$f":"2*3","v":6},"P10KDBCT-ND","ERA-3AEB103V","RES SMD 10K OHM 0.1% 1/10W 0603","MRFS_R10,R13",0.35,2.0999999999999996]
[39,{"$f":"10*3","v":30},"311-10.0KHRCT-ND","RC0603FR-0710KL","RES SMD 10K OHM 1% 1/10W 0603","MRFS_R22,R23,R34,R35,R50,R54,R55,R58,R61,R65",0.015,0.44999999999999996]
[40,{"$f":"1*3","v":3},"541-3645-1-ND","TNPW06032K67BEEA","RES 2.67K OHM 0.1% 1/8W 0603","MRFS_R11",0.65,1.9500000000000002]
[41,10,"RMCF0603JT300RCT-ND","RMCF0603JT300R","RES SMD 300 OHM 5% 1/10W 0603","MRFS_R12,R30,R31",0.013,0.13]
[42,{"$f":"1*3","v":3},"P100KDBCT-ND","ERA-3AEB104V","RES SMD 100K OHM 0.1% 1/10W 0603","MRFS_R14",0.35,1.0499999999999998]
[43,{"$f":"1*3","v":3},"P1.8KDBCT-ND","ERA-3AEB182V","RES SMD 1.8K OHM 0.1% 1/10W 0603","MRFS_R15",0.35,1.0499999999999998]
[44,100,"RMCF0603JT680RCT-ND","RMCF0603JT680R","RES SMD 680 OHM 5% 1/10W 0603","MRFS_R3,R4,R24,R25,R26,R27,R28,R29,R32,R33,R37,R38,R57,R60,R63,R64,R67,R68,R69",0.0051,0.51]
[45,10,"RMCF0603JT1R00CT-ND","RMCF0603JT1R00","RES SMD 1 OHM 5% 1/10W 0603","MRFS_R36",0.013,0.13]
[46,{"$f":"2*3","v":6},"CRE2512-FZ-R003E-3CT-ND","CRE2512-FZ-R003E-3","RES 0.003 OHM 1% 3W 2512","MRFS_R45,R46",0.62,3.7199999999999998]
[47,10,"YAG3565CT-ND","AC0603FR-0712KL","RES SMD 12K OHM 1% 1/10W 0603","MRFS_R47,R51",0.025,0.25]
[48,10,"P2.40KHCT-ND","ERJ-3EKF2401V","RES SMD 2.4K OHM 1% 1/10W 0603","MRFS_R48,R52",0.057,0.5700000000000001]
[49,{"$f":"1*3","v":3},"P120BYCT-ND","ERJ-PA3F1200V","RES SMD 120 OHM 1% 1/4W 0603","MRFS_R66",0.16,0.48]
[50,{"$f":"1*3","v":3},"CKN9087CT-ND","PTS645SK50SMTR92 LFS","RED SWITCH TACTILE SPST-NO 0.05A 12V","MRFS_SW3",0.29,0.8699999999999999]
[51,{"$f":"2*3","v":6},"CKN9085CT-ND","PTS645SH50SMTR92 LFS","GRAY SWITCH TACTILE SPST-NO 0.05A 12V","MRFS_SW1,SW2",0.21,1.26]
[52,{"$f":"36*3","v":108},"36-1033-ND",1033,"TERM TEST POINT LOOP .093\"DIA","MRFS_TP1,TP2,TP3,TP4,TP5,TP6,TP7,TP8,TP9,TP10,TP11,TP12,TP13,TP14,TP15,TP16,TP17,TP18,TP19,TP20,TP21,TP22,TP23,TP24,TP25,TP26,TP27,TP28,TP29,TP30,TP31,TP32,TP33,TP34,TP35,TP36",0.1379,14.8932]
[53,{"$f":"1*3","v":3},"296-37381-1-ND","LM5060Q1MMX/NOPB","High-Side Gate Driver IC Non-Inverting 10-VSSOP","MRFS_U1",2.69,8.07]
[54,3,"296-21834-5-ND","TL2575HV-05IKV","IC REG BUCK 5V 1A TO220-5","MRFS_U2",3.16,9.48]
[55,3,"LM3940IMPX-3.3/NOPBCT-ND","LM3940IMPX-3.3/NOPB","IC REG LINEAR 3.3V 1A SOT223-4","MRFS_U3",1.65,4.949999999999999]
[56,3,"296-44483-1-ND","TMS320F28035PNQR","IC MCU 32BIT 128KB FLASH 80LQFP","MRFS_U4",11.51,34.53]
[57,3,"296-29433-1-ND","DRV8301DCAR","IC MOTOR CONTROLLER SPI 56HTSSOP","MRFS_U5",6.14,18.419999999999998]
[58,3,"620-1722-1-ND","ACS724LLCTR-30AB-T","CURRENT HALL SENSOR BI-DIRECTIONAL 30A AC/DC","MRFS_U6",5.77,17.31]
[59,3,"296-37645-1-ND","OPA2374AIDCNR","IC OPAMP GP 6.5MHZ RRO SOT23-8","MRFS_U7",1.95,5.85]
[60,3,"296-16915-1-ND","SN74LVC3G17DCTR","IC BUFF TRPL SCHMIT TRIG SM8","MRFS_U8",0.72,2.16]
[61,3,"296-44856-1-ND","SN65HVD233QDRQ1","IC TXRX CAN HALF DUPLEX 8SOIC","MRFS_U9",3.25,9.75]
[62,3,"296-24863-1-ND","TRS3232EQPWRQ1","IC DVR/RCV RS232 MULTICH 16TSSOP","MRFS_U10",2.8,8.399999999999999]
[63,3,"535-9046-ND","ABL-20.000MHZ-B2","CRYSTAL 20.0000MHZ 18PF T/H","MRFS_Y1",0.33,0.99]
[64,2,"296-46954-ND","TMDSEMU110-U","XDS110 JTAG DEBUG PROBE","MRFS_JTAG",102.8,205.6]
[65,1,"HM1412-ND","1455Q1601RD","BOX ALUM RED 6.3\"L X 4.92\"W","MRFS_HOUSING",28.99,28.99]

{"sheet":"Sheet1","index":1,"n_rows":10,"n_cols":11,"rows_kept":10,"merged":[[9,0,9,4]]}
["Index","Quantity","Digi-Key Part Number","Manufacturer Part Number","Description","Customer Reference","Unit Price USD","Extended Price USD",null,"Costs"]
[1,4,"MOUSER PN:  926-LM5060Q1MMX/NOPB","LM5060Q1MMX/NOPB","High-Side Gate Driver IC Non-Inverting 10-VSSOP","MRFS_U1",2.91,{"$f":"G2*B2","v":11.64},null,{"$f":"SUM(H:H)","v":67.61},"Subtotal"]
[2,10,"754-1946-1-ND","APTD1608LSECK/J4-PF","LED OR 2mA 1.8V 0603","MRFS_D1,D2,D5,D6,D7,D8,D9,D10,D14,D23,D26,D29,D30,D31,D32,D33",0.476,4.76,null,{"$f":"J2*0.1025","v":6.930025},"Tax (Est)"]
[3,10,"36-575-8-ND","575-8","JACK NON-INSULATED .350\"","MRFS_J2, J3, J4",0.653,6.53,null,{"$f":"10","v":10},"Shipping"]
[4,2,"296-29433-1-ND","DRV8301DCAR","IC MOTOR CONTROLLER SPI 56HTSSOP","MRFS_U5",6,12,null,{"$f":"SUM(J2:J4)","v":84.540025},"TOTAL"]
[5,{"$f":"2","v":2},"296-44483-1-ND","TMS320F28035PNQR","IC MCU 32BIT 128KB FLASH 80LQFP","MRFS_U4",11.89,23.78]
[6,4,"493-15384-ND","UKL1H331KHD","CAP ALUM 330UF 10% 50V RADIAL","MRFS_C15",1.01,4.04]
[7,3,"J147-ND","108-0740-001","CONN JACK BANANA UNINS PANEL MOU","MOTOR PHASE TERMINALS",1.62,4.86]
[]
["NOTE:  ITEM 1 IS OUT OF STOCK FROM DIGIKEY W/ A 22 WEEK LEAD TIME.  WILL NEED TO ORDER FROM MOUSER"]

{"sheet":"Advanced Circuits","index":2,"n_rows":5,"n_cols":10,"rows_kept":5}
["Index","Quantity","Manufacturer Part Number","Description","Customer Reference","Unit Price USD","Extended Price USD",null,"Costs"]
[1,5,"MARS ROVER","REV F PCB","MRFS_PCBF",103.43,{"$f":"F2*B2","v":517.1500000000001},null,{"$f":"SUM(G:G)","v":517.1500000000001},"Subtotal"]
[{"$nulls":8},{"$f":"I2*0.1025","v":53.007875000000006},"Tax (Est)"]
[{"$nulls":8},{"$f":"10","v":10},"Shipping"]
[{"$nulls":8},{"$f":"SUM(I2:I4)","v":580.1578750000001},"TOTAL"]