<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="3" y1="0" x2="67" y2="0" width="0" layer="20"/>
<wire x1="70" y1="3" x2="70" y2="34" width="0" layer="20"/>
<wire x1="67" y1="37" x2="3" y2="37" width="0" layer="20"/>
<wire x1="0" y1="34" x2="0" y2="3" width="0" layer="20"/>
<wire x1="0" y1="34" x2="3" y2="37" width="0" layer="20" curve="-90"/>
<wire x1="70" y1="34" x2="67" y2="37" width="0" layer="20" curve="90"/>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="67" y1="0" x2="70" y2="3" width="0" layer="20" curve="90"/>
<text>S.Harrison</text>
<text>8 April 2018</text>
<text>V1.0</text>
<text>ThingySticks.com</text>
<text>HappySadButtons</text>
<text>+VE</text>
<text>+VE</text>
<text>-VE</text>
<text>-VE</text>
<text>3v3</text>
<text>Switch</text>
<text>LED</text>
<text>3v3</text>
<text>Switch</text>
<text>LED</text>
<text>LED</text>
<text>Switch</text>
<text>3v3</text>
<text>3v3</text>
<text>Switch</text>
<text>LED</text>
<text>3.7V LS16340</text>
<text>ThingySticks.com</text>
<text>HappySadButtons</text>
<text>Stephen Harrison</text>
<text>3v3</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>BME680</text>
<text>+VE</text>
<text>ThingySticks.com/HappySadButtons</text>
<text>GND</text>
<text>3v3</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
<package name="SOT323">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X3">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Tinamous">
<packages>
<package name="PHOTON_SMD">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PTC-1206">
</package>
</packages>
</library>
<library name="ThingySticks">
<packages>
<package name="BATTERY_16340-HOLDER">
<description>Battery holder for LS18340 3.7v Li ion battery</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="1SS355TE-17">
<attribute name="PROD_ID" value="DIO-11623"/>
<attribute name="NAME"/>
<attribute name="FARNELL" value="152-5435"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="1SS355TE-17">
<attribute name="PROD_ID" value="DIO-11623"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="FARNELL" value="152-5435"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X3" value="Left LED Button"/>
<element name="JP2" library="SparkFun-Connectors" package="MOLEX-1X3" value="Right LED Button"/>
<element name="JP3" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="Left Button">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="Right Button">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="U$1" library="Tinamous" package="PHOTON_SMD" value="PHOTON_SMD">
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H2" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT323" value="MOSFET-NCHANNEL2N7002PW">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="NAME"/>
<attribute name="FARNELL" value="189-4713"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X05" value="BME680">
<attribute name="VALUE"/>
</element>
<element name="F5" library="SparkFun-PowerIC" package="PTC-1206" value="1A Max">
<attribute name="PROD_ID" value="RES-08585"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BT2" library="ThingySticks" package="BATTERY_16340-HOLDER" value=""/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="H3" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="RIGHT_BUTTON">
<contactref element="JP2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="16"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="LEFT_BUTTON">
<contactref element="JP1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="U$1" pad="12"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="13"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="14"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="18"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="20"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="22"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="23"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="5"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="10"/>
</signal>
<signal name="LEFT_LED">
<contactref element="U$1" pad="11"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RIGHT_LED">
<contactref element="U$1" pad="15"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="24"/>
<contactref element="S1" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="21"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="BT2" pad="P$2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="V_BATT">
<contactref element="JP3" pad="2"/>
<contactref element="F5" pad="2"/>
<contactref element="BT2" pad="P$1"/>
</signal>
<signal name="BATT_MONITOR">
<contactref element="R1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="BATT_MONITOR_ENABLE">
<contactref element="Q1" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="F5" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
